CLAIRVOYANCE

All TARDIS models use a 4-Dimensional Interstitial Scanning Array linked to their Exo-Chronoplasmic shells to ‘see’ the area surrounding the Real World Interface and beyond. Some models can even see a bit into the future…

Effect

Major Clairvoyance allows the TARDIS scanner to centre their ‘camera’ at any point within a range determined by their Resolve (see table below).

Special Clairvoyance works as above and also reflects the unique ability of some highly experienced or highly advanced TARDIS units to use a Story Point to show images from a short time into the future or past on the TARDIS scanner. These images will have a time differential and a duration based upon the TARDIS resolve (see the table to the right). All TARDIS Units come with this Trait. Enhancing Major Clairvoyance into Special Clairvoyance reduces the TARDIS’ Story Point total by 2.

TARDIS CLAIRVOYANCE
RESOLVE	RANGE	PAST/FUTURE	DURATION
1	5m	30 seconds	Brief flash
2	10m	A minute	1-3 seconds
3	200m	3 minutes	30 seconds
4	1km	5 minutes	A minute
5	10km	10 minutes	3 minutes
6	100km	20 minutes	5 minutes
7	500km	30 minutes	10 minutes
8	1000k	1 Hour	20 minutes
9+	1AU	1 Day	30 minutes